
                      GraphicsENGINE ULTRA Cadvance Driver

 Features:
 * Very Fast-
         Written in 100% assembly language.
 * Very Small-
         Driver uses only 9.0K.

 Hardware Requirements:
 * 286 or better CPU.
 * GraphicsENGINE ULTRA board.

 Resolution:
 * 1280x1024, 1280x960, 1024x768, 800x600, or 640x480.
 * 16 or 256 colors, depending upon monitor and DRAM installed.


               I N S T A L L A T I O N
               -----------------------

 Automatic installation:
 1. Go to disk drive that has Cadvance.
 2. Place the driver install diskette in drive A:.
 3. Type \ A:INSTALL\<CR>.

    Then select INSTALL's \Cadvance Driver \ menu,
    press ENTER key and complete the installation.
    INSTALL will copy the appropriate files to your default directory.


 Manual installation:
 1. Install the driver into a C:\TEMP subdirectory.
 2. Change to the \ \CAD\directory.
 3. Copy  C:\TEMP\CDV911.DRV\to \ GS.DRV\ .
 4. Copy  C:\TEMP\CAD.RND\to \ CAD.RND\ .


               D R I V E R   U S E
               -------------------

 For drivers that do not allow the selection of the resolutions during
 installation, the driver will default to the highest resolution possible.
 If this is not what you desired, the resolution may be overridden by
 setting an environment variable as follows:

 \ set S31_911=<mode>\
 Where <mode> is:
 0     640 x 480, 256 colors
 1     800 x 600, 16 colors
 2     800 x 600, 256 colors
 3     1024 x 768, 16 colors
 4     1024 x 768, 256 colors
 5     1280 x 960, 16 colors
 6     --> reserved <--
 7     1280 x 1024, 16 colors
 8     --> reserved <--

 Please note that not all resolution modes may be available.
 The \ set S31_911=<mode>\instruction can be included in the
 AUTOEXEC.BAT file.

 The driver is loaded into memory by Cadvance, and so requires no
 intervention on the part of the user. Cadvance will also remove the
 driver from memory upon completion, thus conserving DOS memory.

 This driver will work as a rendering device, if sufficient memory
 is installed. The resolution will be the same as the resolution
 used in the 2D and 3D modes. Please note that rendering will only work
 if the driver is currently using a 256 color mode.


