Williams-Renault FW17

Engine:                     Renault V10, RS7, 3.0 litre
                            normally-aspirated
Management System:          Magneti Marelli 
Transmission:               Six-speed Williams transverse
                            semi- automatic 
Clutch:                     AP 
Chassis:                    Carbon Aramid epoxy composite,
                            manufactured by Williams using
                            Fiberite products
Suspension:                 Williams passive 
Steering:                   Williams 
Cooling System:             Two Secan water radiators at 
                            side of chassis; two Secan
                            oil radiators 
Brakes:                     Carbone Industrie disks and pads
                            operated by AP callipers 
Fuel:                       Elf 
Oil:                        Elf 
Wheels:                     Oz; 13*11 front, 13*13.7 rear 
Tyres:                      Goodyear Eagle radials 
Spark Plugs:                Champion 
Cockpit Instrumentation:    Magneti Marelli rev counter with
                            integrated digital data display
                            of key information, including
                            oil and water temperature, fuel
                            consumption and lap time
Seat-belts:                 Six-point Sabelt 
Steering wheel:             Personal 
Driver's Seat:              Anatomically formed in 
                            carbon/epoxy composite material
                            with suede covering 
Extinguisher System:        Williams, with Metron actuators
                            and Zero 2000 extinguishants 
Front track:                1670 millimetres 
Rear track:                 1600 millimetres 
Wheelbase:                  2890 millimetres 
Weight:                     595kg including driver and
                            camera weight 
Car Length:                 4150 millimetres


Renault V10 RS7 Engine

Technical Specification:    10 cylinders in V configuration
                            67 degrees 
Length:                     623mm 
Width:                      540mm 
Height to cylinder heads:   420mm 
Weight:                     approx. 132kg including
                            accessories 
Materials:                  All casings aluminium,
                            reciprocating parts steel or
                            titanium 
Valves:                     Pneumatically controlled

-----------------------------------------------------------
Rothmans Williams-Renault FW17 Specs by Max Galvin
Source: Williams Grand Prix Engineering
