Pacific PRO2
-----------------------------------------------------------

Monocoque:            Combined lay-up of high strength and
                      high mdulas uni-directional carbon
                      fibre skins over aluminium honeycomb,
                      designed in-house using 
                      Hewlett-Packard computer aided desgn
                      systems and manufactured by Advanced
                      Composites. 

Nosebox & Sidepods:   Carbon fibre energy absorbing
                      structures designed to withstand the
                      1995 FIA crash test. 

Engine cover:         Ultra lightweight carbon fibre skins
                      over nomex core. 

Wings:                High modulas carbon fibre female
                      moulded aerofoil sections. 

Aerodynamics:         One-third wind tunnel model developed
                      at MIRA. 

Suspension:           Pushrod,double wishbone/rocker to
                      Penske damper units all round,
                      designed to Pacific's requirements.
                      Fabricated uprights. 

Brakes:               AP 6-pot calipers front, 4-pot
                      calipers rear. Carbone industrie
                      carbon fibre brake disks and pads. 

Engine:               Ford Cosworth ED3.0 litre 75 degreeV8

Telemetry system:     PI `Plus Four' Telemetry system,
                      operating on Hewlett-Packard
                      computers/printers. 

Cooling:              Side-pod-mounted water radiators
                      utilising Secan cores. 

Gearbox:              `Pacific` 6-spead semi-automatic,
                      longitudinal gearbox. Electronically
                      operated gearshift, driver controlled
                      skip shift. 

Oil System:           Pacific designed air/oil radiators
                      supplied by Secan. 

Clutch:               Carbon fibre supllied by AP Racing 

Battery:              Fiamm battery. 

Steering wheel:       In-house Pacific designed, housing
                      electronic driver controls and
                      semi-automatic switch gear and
                      paddles. 

Safety:               6 point driver safety harness. Carbon
                      fibre fire extinguisher system
                      complying to FIA technical
                      regulations.

Wheels:               Dymag, manufactured to Pacific's
                      specifications. 

Fuel Tank:            ATL feul cell manufactured to
                      Pacific's specifications. 


-----------------------------------------------------------
Source: GaleForce Of Monaco