
*******************************************************************
                                                                   
 Copyright (c) Creative Technology Ltd, 1996. All rights reserved. 
                                                                   
*******************************************************************


           CD-ROM INSTALLATION : Latest Information
           ========================================


This file contains information not available during the printing of 
the manual.  Please read its contents before you proceed with the 
installation procedure.

This file contains the following sections :

   1. Running the Installation Program
   2. Updating drivers for Windows 95
   3. MSCDEX driver

			  *****

1. RUNNING THE INSTALLATION PROGRAM

The installation program allows you to set up your CD-ROM drive 
under Windows 3.1/DOS or Windows 95.

To set up your drive in Windows 3.1/DOS, run INSTALL.EXE at the 
DOS prompt.

To set up your drive in Windows 95, run SETUP.EXE in Windows 95.


2. UPDATING DRIVERS FOR WINDOWS 95

To update the drivers required for Windows 95:

a. In the Control Panel folder, double-click the System icon to 
   show the System Properties dialog box.

b. Select the Device Manager tab in the System Properties dialog 
   box.

c. Double-click the appropriate item e.g. "Sound, video and game 
   controllers" to display the devices installed in your system.

d. Double-click the device you wish to update (e.g. Creative 
   Labs Sound Blaster 16 or AWE-32).The Properties dialog box 
   of the selected device appears.

e. Select the Driver tab in the Properties dialog box and choose 
   Change Driver.  The Select Device dialog box appears.

f. Choose Have Disk in the Select Device dialog box.  
   The Install From Disk dialog box appears.

g. Enter the path where the new drivers are located and choose OK. 
   The Select Device dialog box appears.

h. Choose OK to return to the Properties dialog box.

i. Choose OK to exit the Properties dialog box.
   The drivers will be copied to your Windows directory.

j. Choose Close to exit the System Properties dialog box.
   The System Settings Change dialog box appears.

k. Choose OK to restart your system.
	  

3. MSCDEX.EXE DRIVER

   To use your CD-ROM drive under Windows 3.1 or DOS, the 
   Microsoft CD-ROM extension driver (MSCDEX.EXE) must be loaded.

   The installation allows you to search for this driver in your 
   system. It will then copy this driver to your <dir>\DRV directory 
   and place a command in your AUTOEXEC.BAT file to load this 
   driver when your system boots up.

     Note : <dir> is your target installation directory.

   If you do not have the MSCDEX.EXE driver in your system,option 2 
   allows you to add a remarked statement in the AUTOEXEC.BAT file.  
   If you do so, you will then need to obtain this driver from your 
   vendor and copy it to your <dir>\DRV sub-directory.  Finally, 
   remember to remove "REM" from the command that loads the 
   MSCDEX.EXE driver in the AUTOEXEC.BAT file.  


         **********  E N D   O F   R E A D M E  **********
