Archtek Introduces Combination V.32 Terbo
Voice/Fax/Modem/Speakerphone/Answering Machine

CITY OF INDUSTRY, Calif -- Archtek America Corp., manufacturer of external,
internal and PCMCIA cards and other fax/modems, has added the 19.2Kbps
ConferencePal V.32 terbo Voice Fax Modem with Speakerphone to its
SmartLink line of products. This internal card automatically distinguishes
between data, fax and voice transmissions, and offers state-of-the-art
technology with advanced features to provide high-speed performance,
maximum flexibility and optimum reliability. 

The SmartLink ConferencePal is bundled with a specially developed
voice/fax/modem software, which provides a complete, easy-to-use
telecommunications management system for Windows 3.1, Windows 95 or DOS
6.2 or beyond. 

This new Archtek product is compatible with virtually all fax/modems and
fax machines. Combined with the answering machine feature, it supports
broadcast fax and fax-on-demand. The modem transfers data up to 19,200bps,
by adding V.42bis MNP 5 data compressions the throughput increases up to
76,800bps. 

In addition to the standard way of answering a telephone, with
ConferencePal, the user has the option of clicking an icon and responding
via the speakerphone. With this hands-free voice response, the user can
continue working on other applications without the necessity of picking up
the telephone. In combination with a separate, full-duplex speaker and the
Archtek microphone, the user is assured of static-free communications.
Plus, the microphone can be moved to a spot convenient to the user. This
unique communication feature is ideal for desktop teleconferencing,
including communicating to locations across the world. 

The full-featured answering machine/voice mail can be accessed locally or
remotely, and will record digitized greetings and voice messages for up to
ten personalized mailboxes. It both records and plays back using 8- or 16-
bit audio data at 7.2KHz, 8.0KHz or 11.025KHz. And it supports EIA/TIA
IS-101 AT+V voice command, along with 8-bit U-law or A-law compression at
8.0KHz. 

The SmartLink ConferencePal is designed to meet the V.32 bis international
standard. Conforming to the characteristics of the connection by first
probing the channel, then setting the frequency, equalization, symbol rate
and transmitted power to maximize data transfer speeds. Based on the
fall-forward and fall-back intelligence, the modem will automatically
adjust to a higher or lower speed, ensuring a clear, precise connection. 

SmartLink ConferencePal has a very low MSRP of only $149, and it is backed
by a limited five-year warranty. For further information, contact Archtek
America Corp.; 18549 Gale Avenue; City of Industry, CA 91748; Tel: (818)
912-9800; Fax (818) 912-9700. 30-30-30
 
 =========================================================
 From the 'New Product News' Electronic News Service on...
 AOL (Keyword = New Products) and Delphi (GO COMP PROD)
 =========================================================
 This information was processed from data provided by the
 company/author mentioned. For additional details, please
 contact them directly at the address/phone# indicated.
 Trademarks are the property of their respective owners!
 =========================================================
 All submissions for this service should be addressed to:
 BAKER ENTERPRISES,  20 Ferro Dr,  Sewell, NJ  08080  USA
 Email:   rbakerpc@aol.com   --or--   rbakerpc@delphi.com
 =========================================================
