*
* Printer Definition for EPSON DX20/35 and Diablo 630
*
*--------------------------------------------------------------------
* The following options are set immediately.  They are not activated
* by parameters.
*--------------------------------------------------------------------
PRINTER: EPSON DX20/35 and Diablo 630
LETTER			* LETTER QUALITY Daisy Wheel
TOPMARGIN 0
BOTMARGIN 0
LINELEN 80
LINESPAGE 66
*MICSPACE 27 65 9	  * SET MICRO SPACING to n 72nds of an inch
*FORMLEN 27 67 66	  * set form length in lines  66 = 66 lines
*FORMLENI 27 67 0 11	  * Set form length in inches 11 = inches
FFEED 12		* Form Feed Character
*--------------------------------------------------------------------
* The following parameters are activated by parameters
*--------------------------------------------------------------------
EMPH 27 79
EMPHOFF 27 38
*DOUBLE 27 71		    * double strike (nlq) printing
*DOUBLEOFF 27 72
*NLQ 27 73 2
*NLQOFF 27 73 0
*DLFONT 27 37 1 0	  * Download font off
*DLFONTOFF 27 37 0 0
*PERFSKIP  27 78 4	  * set number lines to skip over perfs (4)
*PERFSKIPOFF 27 79
ONEDIR 27 92		 * print in only 1 direction
ONEDIROFF 27 47
8LPI 27 82 83 6
6LPI 27 82 83 8
*CHARSET 27 54		  * Select char set 2	27 55 = char set 1
*CHARSETOFF 27 55
*12CPI 27 77		  * 12 characters per inch
*12CPIOFF 27 80
*
* FUTURES ------------------------------------------------------
*
PITCH 27 85 83 NNN	 * HMI --  DISTANCE BETWEEN CHARS IB 120TH INCH
PITCHOFF 27 83		 * RESET TO DEFAULT PITCH

PROPORTIONAL 27 80
PROPORTIONALOFF 27 81

AUTOJUST 27 77		 * ADJUST SPACES BETWEEN WORDS
AUTOJUSTOFF 27 88

