*
* Printer Definition for IBM's ProPrinter
*
PRINTER: IBM's ProPrinter
TOPMARGIN 0
BOTMARGIN 0
LINELEN 80
LINESPAGE 66
*
DOT                     * DOT LETTER LASER
COMPON 15               * set compressed print
COMPOFF 18
FFEED 12                * Form Feed Character
EXPAND 14               * SET EXPANDED PRINT
EXPANDOFF
*MICSPACE 27 65 9         * SET MICRO SPACING to n 72nds of an inch
*FORMLENL 27 67 66         * set form length in lines  66 = 66 lines
*FORMLENI 27 67 0 11      * Set form length in inches 11 = inches
EMPH 27 69
EMPHOFF 27 70
DOUBLE 27 71               * double strike (nlq) printing
DOUBLEOFF 27 72
NLQ 27 73 2
NLQOFF 27 73 0
DLFONT 27 73 4           * Download font off
DLFONTOFF 27 73 0
PERFSKIP  27 78 4        * set number lines to skip over perfs (4)
PERFSKIPOFF 27 79
ONEDIR 27 85 1           * print in only 1 direction
ONEDIROFF 27 85 0
8LPI 27 48
6LPI 27 50
CHARSET 27 54            * Select char set 2   27 55 = char set 1
CHARSETOFF 27 55
12CPI 27 58              * 12 characters per inch
12CPIOFF 18
