CSF disk images (3.5 inch) for ALL WARP and newer 2.11 FixPaks
______________________________________________________________
(German)

Corrective Service Facility disks for installing OS/2 FixPaks.

The images are in LOADDSKF format and require LOADDSKF.EXE to
create two diskettes.

Create TWO 'Kicker' diskettes from this and keep for the Fixpaks.

     WKICKRGR.ZIP *  Contains CSFBOTGR.1DK and CSFBOTGR.2DK and a
                     README.TXT.


Installation
____________
Place a blank, formatted 1.44MB diskette in A: (or B:, whichever
is your 3.5inch floppy drive).

Enter LOADDSKF CSFBOTGR.1DK A: to create the 1st diskette

Place another blank, formatted 1.44MB diskette in the same drive.

Enter LOADDSKF CSFBOTGR.2DK A: to create the 2nd diskette

Save these diskettes for use when installing any OS/2 3.0 (Warp)
or any OS/2 2.11 Fixpak starting with XRxA096 or later.


NOTE: CSFBOTGR.1DK contains the German version of readme file
      which is in an INF format, README.INF.  To view the readme
      file type:
                 VIEW README.INF
      at command prompt in an OS/2 Window.
