*********************************************************************************
                                  ipPulse
              Welcome to ipPulse 1.20 Trial Version "readme" file
               (c) 1998-2000 Northwest Performance Software, Inc.
*********************************************************************************

--------------
DOCUMENT INDEX
--------------
This file contains the following sections:

1. General Notes
2. Contact Information
3. Installation Instructions
4. Revision History
5. Client Function Summary

*********************************************************************************
GENERAL NOTES

Program Requirements.
*Windows NT 4.0 Workstation or Server, 2000 or Windows 98. It will
run on Windows 95 with the winsock 2 update.
(all the preceding are trademarks or registered trademarks of the
Microsoft Corporation).
*Requires Winsock 2
*Approximately 2.7 MB disk space
*TCP/IP Network connection with DNS

License Agreement.
Please see license.txt

Purchase Cost.
$69 on CDROM only. Shipping is extra. Please see our website for the most current
pricing and shipping information:
http://www.ippulse.com/ippulsemain.html

Suggestions/Comments/Bug Reports
Please email all suggestions/comments/bug reports to:
sales@nwpsw.com

*********************************************************************************
CONTACT INFORMATION

email:			sales@netscantools.com or sales@nwpsw.com
WWW-main site:		http://www.nwpsw.com/index.html
			http://www.ippulse.com/ippulsemain.html

Mailing address:
Northwest Performance Software, Inc.
PO Box 148
Maple Valley, WA 98038-0148 USA

Telephone.  VOICE: (253) 630-7206 (8am to 5pm Pacific (Seattle-LA) Time)
24 hour/7 day FAX: (253) 639-9865

*********************************************************************************
INSTALLATION INSTRUCTIONS

1. If this file was zipped. Unzip and copy all files to a new,
   empty directory (folder).
2. Close this file.
3. Run setup.exe from your preferred file management program.
 Be sure to install this program in a directory different than the directory
 created in step 1 above.
4. Follow the instructions in the setup program.

*********************************************************************************
REVISION HISTORY

1.20 Release 2/9/00
	Fixes
	*Removed IP to host resolution in SMTPMAIL.
	*Improved threading.
	*Ping min and max times now correctly reflect the min and max times
	occurring during a run/stop session.

	Additions
	*Moved several things from Primary Test setup page to new Setup/Program
	Control page.
	*Added cycle control. Either infinite or fixed number of passes through
	the target list.
	*Added control to set number of times to attempt hostname/ip address
	resolution.
	*Added Edit Column Visibility feature. This controls which columns are
	visible.
	*Added ability to reset primary and secondary pass and failure counts.
	*Added Ping Average time column.
	*Added Failure Count Trigger Point control to Failure Criteria tab.
	*Added ability to send error messages to multiple pagers on the same
	pager provider. One call to the provider can trigger several pagers.
	*Improved help file and switched to a different HTML help method.

1.11 Release 11/04/99
	Fixes
	*Several minor cosmetic fixes such as graying out boxes at the right time,
	tooltips for the new small extended menu buttons on the main page.
	*Deactivating the extended menu buttons on the main page during a RUN cycle.
	*Pager Phone Number entry dialog box now has column titles that change to
	reflect whether a numeric or alphanumeric pager is being setup.

	Additions
	*Separated Email Max Alerts from Pager Max Alerts on the Setup/Failure Alerts
	tab. Remote Control now displays both alert counts separately.

1.10 Release 7/30/99
	Fixes
	*Algorithm to automatically add 1 second to SNMP query timeout upon no response
	 was removed.
	*Now using pager DLL PowerPage version 2.07b.
	*Hostname/IP address resolution now done using the same thread function as is
	 used in NetScanTools Pro 2000.
	*Shutdown of threads during testing improved.
	*SNMP now updated to 3.6.1.

	Additions
	*Colorized PASS/FAIL rows. Colors can be set on the Setup/Define Display Colors
	 tab.
	*Autostart on program start. To activate, see the Setup/Primary Test tab.
	*Complete overhaul of the Target List Editor. Now includes fields for separately
	 specifying the unique SNMP Community Name, Primary and Secondary TCP Ports and
	 comments for each target. IP Address Range Generation. Clear Target List.
	*Comments column, editable from the Target List Editor.
	*PASS/FAIL test count columns for each of the tests, primary and secondary.
	*Last test FAIL time columns for each of the tests, primary and secondary.
	*Two new buttons below the Exit button activate a new set of buttons:
	 -AutoSize, which will size the column widths to the longest text string.
	 -Print/Save, which allows you to print or save the results area information.
	 -Logs, which allows you to view the Error, Test, and SMTP email logs.
	 -News, which launches your web browser to view the latest ipPulse news.
	*Log files now have formatting change: we now include hostname after IP address
	 and the comments column is included after the hostname.
	*Email messages include the hostname and comments because the email message body
	 gets the same data as the log file.
	*Email messages can optionally show the first 100 characters of the log file
	 error message in the subject line. See Setup/Failure Alerts/Email Setup.
	*Email messages can now have multiple recipients.

1.05 Update 6/1/99
	Fixes
	*Email Notifications now have the subject line filled in properly.

1.04 Update 5/21/99
	Fixes
	*Fixed a pager bug where if your modem was in use and pager alerts were enabled,
	 and ipPulse tried to use the pager, it would get hung up trying to send the
	 page and also create a large pager.log file. Now, if the modem is in use, it will
	 try 6 times waiting 5 seconds between each try. Errors are logged to pager.log.
	*Fixed a problem with snmpwalk where it could have crashed under certain limited
	 circumtances.

1.03 Update 5/11/99
	Fixes
	*Spawned SNMP walk processes now have a 60 second maximum lifetime.
	*SNMP walk has now been version updated to UCD 3.6.1.
	*Top of target list is now visible when program is started.
	*Paging Setup and Email Setup now properly launch HTML help.

	Additions
	*When a row in the main window is selected, it is now highlighted all
	 the way across the row.
	*A program can now be launched upon failure. You must assure that the
	 program you launch is self-terminating.
	*The target number of the failed target can now be sent to a numeric
	 pager. See Paging Setup.
	*Help file updated.

1.02 Update 4/6/99
	Fixes
	*Text changed on percentage returned packets to correctly reflect how
	 the PASS/FAIL triggering actually works.
	*All dialog box text checked to ensure that text clipping is eliminated.
	*Tab key ordering in all dialogs corrected.
	*Log files now include tab character formatting for easier import into
	 spreadsheets and databases.

	Additions
	*Pager setup now includes control of the specific TAPI/COM port used and
	 includes modem init string control. Pager modem logging was also added.
	*Help file updated.

1.01 Update 1/5/99
	Fixes
	*AlphaPager now correctly appends the error message to the header when
	sending an alphanumeric error page.
	*Memory leaks due to premature thread termination fixed.
	*Duplicate <BODY> tag removed from error web page generator.

1.00 Release Version 10/9/98

*********************************************************************************
Client Function Summary

ipPulse (a Remote Status Monitor) is an application used to monitor the active
status of any number of TCP/IP connected computers. Any loss of connectivity
can be logged and a person notified audibly, or through any other number of means
such as email, or a dynamically created web page.

To use ipPulse, do the following:
1. Start ipPulse
2. Press the Help button and follow the Getting Started section

2/9/00
[end]
