SUNET

S Address: UNET Umea Computing Center S S-901 87 Umea WEDEN

E-mail: sunet-staff@sunet.se (Operations staff)

D

Phone: +46 90 16 61 00 (Hans Wallberg)

escription SUNET, or the Swedish University Network, interconnects local and regional networks at b universities in Sweden. The goal of SUNET is to provide good data communications that are eneficial to the universities. The network is used by researchers and teachers of all discip- - m lines. SUNET provides Swedish academic and research users with network resources for com unications both within Sweden and around the world through electronic mail, remote login, S file transfer, and other methods.

UNET is a protocol-independent network based on Ethernet (IEEE 802.3) interconnections. o Currently only IP and DECnet (and EARN) are carried over the backbone. The configuration f SUNET is a backbone star network centered at KTH in Stockholm with 64 kbps lines inter- r connecting the local Ethernets to one nation wide Ethernet. The lines are interconnected via emote bridges (Vitalink). Routers are used to support the various protocols: Cisco for IP and T VAXes for DECnet (and EARN). SUNET also maintains a separate X.25 network. here are two interconnected central mail hubs, one for IP/SMTP, RSCS/BSMTP and T VMS/Mail and one for EAN/X.400 mail.

here are (at least) 3000 IP hosts and 650 DECnets in SUNET. • SUNET has international connections to

EARN (via NORDUnet) • • EUnet via NORDUnet

HEPnet via NORDUnet • • NORDUnet

NSFNET via NORDUnet • • SPAN via NORDUnet

EANnet s I Network Acces t is possible for any IP host on the Internet to access SUNET.

S Who Can Use the Network UNET may only be used for academic and research traffic.

January 29, 1990 NNSC Section 5.28, Page

Miscellaneous Information . F See also the information about NORDUnet or more information about SUNET contact: e B Hans Wallberg, Manager +46 90 16 61 00 hwg@umdc.umu.s jorn Eriksen, Head of operations +46 8 790 6513 ber@sunet.se

January 29, 1990 NNSC Section 5.28, Page