             INSTALL OS/2 2.1 for a B: 3 1/2" diskette
           for the COMPRESSED version (SALMON diskettes)

You will find 2 files in the package. You will ONLY need them if your
ORIGINAL diskettes are SALMON colored. If they are BLUE, you need the
INS21L.ZIP file.

These are 5.25" diskette images of the install disk and disk 1 for installing
from B where the user has a 5.25 A drive but a 3.5 B drive.

You will also need the IBM LOADDF.ZIP file as that utility is need to
uncompress the .DSK files. Create the 5 1/4" diskettes from the following
DSK images, and then boot the system with the INS diskette, and follow
directions. You will need to use both drives, the newly created ones in the
A: drive, and the original shipped 3 1/2" diskettes in the B: drive.

INSTL_M  DSK  1049200   6-16-93   1:01p <--- Install Diskette
BINSTL_M DSK   884240   6-16-93  12:58p <--- Diskette #1
