NOTE: Users of QEMM from Quarterdeck who are using the LOADHI.SYS 
feature to locate device drivers into high memory areas may, in 
very rare instances, experience a lock-up when exiting this demo.  

If this problem occurs, it can be avoided in the future by 
adding the option NOVIDEORAM to the QEMM statement in the 
CONFIG.SYS file; consult your QEMM manual for more information.
