KEYWORDS MUST BE FOLLOWED BY AN EQUAL SIGN FOLLOWED BY ESCAPE SEQUENCE
CONTROL SEQUENCES ARE TERMINATED BY A \41
KEYWORDS MAY OCCUR IN ANY ORDER;ONLY THE LAST OCCURENCE WILL BE RECORDED
AN EQUAL SIGN SHOULD NOT OCCUR IN THE ESCAPE SEQUENCES
NON CHARACTERS ARE INDICATED BY \ FOLLOWED BY HEX VALUE
		IBM PRINTER
width		=8
topbit		=7
setup  		=\1B@\1b3\18\41
header		=\1bL\D0\02\41
tail		=\0d\0a\41
restore		=\1b@\40\41
normal		=1
normal alt	=2
reverse		=3
reverse alt	=4
normal both	=5
reverse both	=6
