
>>> Visit our Home Page at www.cdrunner.com!

                     CD-Runner 6.0 DeLuxe Requirements

CD-Runner 6.0 is compatible with Windows 95 and Windows NT 4.0. 

We recommend the following as a nominal environment for using CD-Runner:

(Note: It is highly recommended that CD-Runner be installed on MMII-class
[multimedia 2] PCs. This will render both the highest performance of
CD-Runner, as well as current CD-ROM application discs.

   * Pentium class 60 MHz or better IBM-compatible computer. CD-Runner 
     may also be run on 486 processors, provided that they are DX-2 and 
     100 mHz or better.
   * Windows Version 95 or later, or Windows NT 4.0 or later.
   * Mouse.
   * 8 MB RAM or greater.  16 MB or better is recommended for optimal 
     multimedia performance.
   * One hard disk drive, one MCI-compatible IDE or SCSI CD-ROM drive.
   * Sound card. Sound-Blaster compatible is recommended.
   * Approximately 5 MB available hard disk space.
   * Windows 95 MCI CD player compatible driver and driver for CD Audio. 
     These are automatically installed during Window 95 Setup, but may not
     be resident if you have overinstalled Windows 95 as an upgrade to 
     Windows 3.x.  This is rare, and if you are able to run audios via the
     Microsoft CD Player, most unlikely.
   * It is HIGHLY recommended that you NOT have mscdex.com loaded in your 
     autoexec.bat, but rather let Windows 95 set up your CD-ROM drive(s).
     (Mscdex.com is a DOS driver that can seriously slow down Windows 95 
     CD-ROM performance.)
   * Highly Recommended: Modem w/Internet hookup.

---------------------------------------------------------------------------
CD-Runner is a registered trademark of Beyond Software.
CD-Runner copyright 1995-1997 Beyond Software. All rights reserved worldwide.
CD-Runner is produced and distributed exclusively by ISS
  - Integrated Software Systems.
Other products and companies referred to herein are trademarks or registered 
  trademarks of their respective companies or mark holders.

                                     <end>
