ACECAD Announces Release of Professional High Precision 12" X 12" D-9000+ &
12" X 18" D-8000 Pro Digitizer Tablets

Monterey, CA - ACECAD Inc., manufacturer of a comprehensive range of
digitizers, announces two new additions to the D-Series product line. The
new 12" X 12" D-9000+ and the 12" X 18" D-8000 Pro tablets represents
ACECAD's latest generation of easy to use, high performance and high
resolution graphic input devices. Both tablets offer a unique five
emulation memory storage capability, built-in "easy-set-up" point and
click template and dual transducer port allowing simple one-time dual port
plug in for both the included two button pen and four button puck
transducer devices. (A unique swivel head 16 button puck is optionally
available). These two new tablets are designed for maximum ease of
installation and use for professionals as well as first time digitizer
users.

Both tablets can be used for a wide range of applications, including:
animation, architecture, computer-aided design (CAD), desktop publishing,
drafting, graphic arts and illustration, mapping, presentation graphics,
and other industrial, business and home applications. In addition, all
tablets work with the latest pen-centric applications in the new pen based
computing environments.

Advanced Technology

All D-Series tablets are PC and/or Macintosh compatible and feature the
most advanced electromagnetic inductive technology. In the both the PC and
MAC environments, the new tablets provide a critical pin-point accuracy of
+/-0.01" and supports resolutions of up to 1016 LPI, greatly reducing
jitter and vastly increasing the stability of the tablet.

Easy To Use

ACECAD digitizers are the easiest tablets to set-up and use and offer the
best Tablet values in the marketplace today. Three advanced features make
the D-Series perfect for home, classroom or corporate environments where
multiple users operate on the same digitizer. These features are:

-- A unique point-and-select configuration template offering up to five
emulation capabilities allowing for extremely easy set-up and use. The
template, which is built right on the tablet surface, sharply decreases
work time by allowing the user to quickly and easily configure the tablet
to their desired emulation, freeing them from time consuming adjustments
when changing applications. Configuring the tablet is simplified by a LED
located in the upper right-hand corner of the tablet which lights up as
the stylus or puck is moved over the parameters which the tablet is
currently configured as.

-- Five emulation memory storage capability which allows the user to easily
and quickly store up to five different application configurations.
Switching from one emulation to another is as easy as point-and-select,
and configurations can be saved for later use. This feature enables users
to move quickly and easily from AutoCAD to DOS or Windows and back to
AutoCAD without powering down, changing dip switches or unplugging
cables.

-- A unique dual transducer port which allows both the included cursor/puck
and stylus pen to always be active, giving the user the freedom to easily
switch back and forth between the two tools without disconnecting one to
use the other.

What's Included

Each D-9000+ & D-8000 PRO tablet includes a 4-button cursor puck, 2-button
stylus pen, AutoCAD 10, 11 or 12 templates, RS-232 serial interface cable,
anti-static dust cover, and Comprehensive User's Manual. Also included are
specialized drivers for a wide variety of applications, including an AADI
real mode and protected mode driver suite for Autodesk applications; an
ATABLET.COM mouse driver which provides absolute mouse emulation for
applications in DOS requiring Microsoft Mouse emulation; simply swap from
DOS to Windows and back again with ease; an ATEST.EXE driver which
provides the user with the ability to simply plug the tablet into a serial
port and quickly verify communications between the tablet and computer,
and an all new WinTab driver contains a custom tablet control panel
utility for use under Windows 3.X. This driver suite lets the user utilize
the included WinTab Tablet Control Panel program to customize the size of
the tracking area on the tablet surface corresponding to the whole Windows
screen so pointing and selecting and menu-picking become as easy as slight
wrist rotation. The WinTab Tablet Control Panel also lets you control the
sensitivity of the tablet, the tablets aspect ratio and even customize
button configurations such as left click, left double click, left drag,
right click, etc. on the included stylus pen or cursor puck. You can even
install two pointing devices in Windows using this versatile new driver.
Also included is an autoinstall program making install a breeze. In
addition, a built-in self diagnostics test checks all critical components
and hardware each time the tablets are powered on. A 16-button cursor puck
with adjustable cross-hairs for optimum right or left hand usage is
available as an optional accessory.

All D-Series tablets are backed by a three year tablet warranty and a one
year accessories warranty, and are developed and manufactured in our own
facilities using only the most advanced electromagnetic inductive
technology. Maintaining complete control over the engineering, production
and distribution functions has enabled ACECAI) to produce the highest
quality digitizers at the lowest possible prices.

ACECAD Inc
PO BOX 431
Monterey, CA 93942-0431

2600 Garden Rd, Suite #121
Monterey, CA 93940

1-800-676-4ACE,   408-655-1900,   FAX: 408-655-1919
BBS: 408-655-1988,  Technical Support: 408-655-9911

 ============================================================
 From the  'New Product Information'  Electronic News Service
 on AOL (Keyword = New Products) & Delphi (GO BUSINESS PROD)
 ============================================================
 This information was processed from data provided by the
 above mentioned company. For additional details, contact 
 the company at the address or telephone number indicated.
 OmniPage Pro is now used for converting all printed input! 
 ============================================================
 All submissions for this service should be addressed to:
 BAKER ENTERPRISES,  20 Ferro Dr,  Sewell, NJ  08080  U.S.A.
 Email: RBakerPC (AOL/Delphi), rbakerpc@delphi.com (Internet)
 ============================================================
