   Note for SoundBlaster 16 and AWE32
   תתתתתתתתתתתתתתתתתתתתתתתתתתתתתתתתתת

     There is a bug in Midas Sound System v0.32c which disables auto-detect 
  of SoundBlaster 16 and AWE32 cards. You will have to use the command line 
  which can feed in the correct port, irq and dma. Use MAZPLAY -H to list 
  the command line parameters.

     For Example: 
     
     MAZPLAY -s4 -o8s -v64  
     
     (PUT VOLUME AT 64, IT STARTS AT 20 (for GUS Users))
     (AND AT 20 IT SOUNDS LIKE CRAP ON SB)
                                              
     WHEN IN SONGS THAT ARE PLAYING USE THE + / - KEYS TO ADJUST THE                                         
     VOLUME TO 64.  IT IS SET AT 20 FOR GUS USERS.


                                              rollo
