Information for Tseng Chipset Users

The XFree86 Project, Inc. 13 November 1994

Contents

1 Supported chipsets 1

2 Clock selection problems with some ET4000 boards 1

3 Text mode restore problems 2

1 Supported chipsets

The Tseng chipsets supported by XFree86 are ET3000, ET4000, and ET4000/W32. At this time, the accelerated features of the ET4000/W32 are not supported; the chipset is treated as a standard ET4000. For details about the accelerated ET4000/W32 server, refer to README.W32 (W32.html).

2 Clock selection problems with some ET4000 boards

XFree86 has some problems getting the clock selection right with some ET4000 boards when the server is started from a high-resolution text mode. The clock selection is always correct when the server is started from a standard 80x25 text mode.

This problem is indicated when the reported clocks are different when the server is started from the highresolution text mode from what they are when it is started from the 80x25 text mode. To allow the server to work correctly from the high-resolution text mode, there are some Option flags that may be set in XF86Config. To find out which flags to set, start the server with the -probeonly flag from an 80x25 text mode and look at the information printed by the server. If the line:

VGAXXX: ET4000: Initial hibit state: low

is printed, put the following in the SVGA, VGA16 and VGA2 sections of your XF86Config:

Option "hibit_low"

If the line:

VGAXXX: ET4000: Initial hibit state: high

3. Text mode restore problems 2

is printed, put the following in the SVGA, VGA16 and VGA2 sections of your XF86Config:

Option "hibit_high"

3 Text mode restore problems

In XFree86 1.3, an option flag “force bits” was provided as an experiment to attempt to alleviate textrestoration problems that some people experienced. We have now made the behavior of this option the default, hence the flag has been removed. Hopefully the past text-restoration problems are alleviated in XFree86 2.0.

$XConsortium: tseng.sgml,v 1.2 95/01/23 15:34:58 kaleb Exp $
$XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/tseng.sgml,v 3.4 1995/01/28 16:03:19 dawes Exp $